;**********************************************************
; Copyright 2004 -2005 TechnoTrend AG
;
;	- TT7146KS.inf
;	- PCI Bridge SAA7146 KS WDM Capture Driver
;
;**********************************************************


[Version]
Signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%TechnoTrend%
;CatalogFile=TT7146KS.cat
DriverVer=02/17/2005, 3.8.0.3
; für Win9x notwendig
LayoutFile=layout.inf

[Manufacturer]
%TechnoTrend%=TechnoTrend

; für Win9x notwendig, kann evtl. entfallen
[PreCopySection]
HKR,,NoSetupUI,,1


[TechnoTrend]
%TTDVBPCI.DeviceDesc_S_HA% = TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_000313c2
%TTDVBPCI.DeviceDesc_S_GL% = TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_000413c2
%TTDVBPCI.DeviceDesc_S_TS% = TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_000513c2
%TTDVBPCI.DeviceDesc_S_TT% = TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_000013c2
%TTDVBPCI.DeviceDesc_S_TT% = TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_100213C2
%TTDVBPCI.DeviceDesc_T_TT% = TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_000113c2
%TTDVBPCI.DeviceDesc_T_TT% = TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_000813c2
%TTDVBPCI.DeviceDesc_C_TT% = TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_000213c2
%TTDVBPCI.DeviceDesc_C_SN% = TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_0000110a
%TTDVBPCI.DeviceDesc_C_OC% = TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_000913C2
%TTDVBPCI.DeviceDesc_C_OC1%= TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_000A13C2
%TTDVBPCI.DeviceDesc_S_OC% = TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_000B13C2
%TTDVBPCI.DeviceDesc_T_OC% = TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_000C13C2
%TTDVBPCI.DeviceDesc_S_TT% = TT7146KS.Device.NT, PCI\VEN_1131&DEV_7146&SUBSYS_000E13C2


[SourceDisksNames]
1=%DiskName%,,

[SourceDisksFiles]
TT7146KS.sys = 1
ttloophe.inf = 1
ttloophe.sys = 1
readme.txt = 1,DrvSetup\Win98
cinstall.exe = 1,DrvSetup\Win98

[SourceDisksFiles.x86]
TT7146KS.sys = 1
ttloophe.inf = 1
ttloophe.sys = 1
fastinst.exe = 1,DrvSetup\Win2000

[DestinationDirs]
TT7146KS.CopyDrivers = 10,system32\drivers
TTLoopHeFiles = 10,temp\TTSetup
TTLoopHeFiles.NT = 10,temp\TTSetup

[TT7146KS.Device]
Include		= ks.inf, kscaptur.inf,ksfilter.inf
Needs		= KS.Registration,KSCAPTUR.Registration
CopyFiles	= TT7146KS.CopyDrivers, TTLoopHeFiles
AddReg		= TT7146KS.AddReg, TTLoopHe.AddReg

[TT7146KS.Device.NT]
Include		= ks.inf, kscaptur.inf, ksfilter.inf
Needs		= KS.Registration,KSCAPTUR.Registration.NT
CopyFiles	= TT7146KS.CopyDrivers, TTLoopHeFiles.NT
AddReg		= TT7146KS.AddReg, TTLoopHe.AddReg.NT

[TT7146KS.Device.NT.Services]
Addservice = TT7146KS, 0x00000002, TT7146KS.AddService

[TT7146KS.AddService]
DisplayName    = %ServiceDesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_DEMAND_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\TT7146KS.sys

[TT7146KS.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,TT7146KS.sys
HKR,,PageOutWhenUnopened,3,0
HKR,,DontSuspendIfStreamsAreRunning,3,01

HKR, "Parameters", "EnableXBar"    	,,"0"
HKR, "Parameters", "EnableXport"   	,,"0"
HKR, "Parameters", "EnableDebi"    	,,"0"
HKR, "Parameters", "EnableMPEG"    	,,"0"
HKR, "Parameters", "SwitchInputPort"    ,,"0"
HKR, "Parameters", "SyncSelPortA"  	,,"A"
HKR, "Parameters", "SyncSelPortB"  	,,"B"
HKR, "Parameters", "AutoAdjustHyo" 	,,"0"
HKR, "Parameters", "InvertField"   	,,"1"
HKR, "Parameters", "IsITU656Input"   	,,"1"


[TTLoopHe.AddReg]
HKLM,%Reg_TT_RunOnce%,TTSetup,,%10%"\temp\TTSetup\cinstall.exe -c""Net"" -m""TechnoTrend AG"" -d""Virtual DVB-S/-C/-T Network Adapter"" -i""%10%"\temp\TTSetup\"""

[TTLoopHe.AddReg.NT]
HKLM,%Reg_TT_RunOnce%,TT_Setup,,%10%"\temp\TTSetup\fastinst.exe "%10%"\temp\TTSetup\ttloophe.inf"


[TT7146KS.CopyDrivers]
TT7146KS.sys

[TTLoopHeFiles]
ttloophe.inf
ttloophe.sys,,,2
readme.txt
cinstall.exe

[TTLoopHeFiles.NT]
ttloophe.inf
ttloophe.sys,,,2
fastinst.exe


[TT7146KS.Device.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,

[TT7146KS.Device.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,

[VideoCapture]
AddReg=VideoCapture.AddReg

[VideoCapture.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%Desc.Filter%


;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]
SERVICE_KERNEL_DRIVER=1
SERVICE_ERROR_NORMAL=1
SERVICE_AUTO_START=2
SERVICE_DEMAND_START=3

TechnoTrend		= "TechnoTrend AG"
DiskName		= "TechnoTrend DVB/PCI Driver & Software CD-ROM"
ServiceDesc		= "TechnoTrend SAA7146 Capture (WDM)"
Desc.Filter		= "TechnoTrend SAA7146 Capture (WDM)"

TTDVBPCI.DeviceDesc_S_HA = "Hauppauge WinTV-Nexus (KS)"
TTDVBPCI.DeviceDesc_S_GL = "Galaxis DVB PC-Sat-Karte (KS)"
TTDVBPCI.DeviceDesc_S_TS = "Technisat SkyStar 1 (KS)"
TTDVBPCI.DeviceDesc_S_TT = "TechnoTrend TT-PCline premium S (KS)"
TTDVBPCI.DeviceDesc_T_TT = "TechnoTrend TT-PCline premium T (KS)"
TTDVBPCI.DeviceDesc_C_TT = "TechnoTrend TT-PCline premium C (KS)"
TTDVBPCI.DeviceDesc_C_SN = "Siemens C (KS)"

TTDVBPCI.DeviceDesc_C_OC = "Octal DVB-C + Analog (KS)"
TTDVBPCI.DeviceDesc_C_OC1= "Octal DVB-C + Analog Rev. 1.1 (KS)"
TTDVBPCI.DeviceDesc_S_OC = "Octal DVB-S (KS)"
TTDVBPCI.DeviceDesc_T_OC = "Octal DVB-T (KS)"

Reg_TT_RunOnce="Software\Microsoft\Windows\CurrentVersion\RunOnce"
