AIRTUN-NG(1)

NAME
airtun-ng - a virtual tunnel interface creator for aircrack-ng

SYNOPSIS
airtun-ng [options] <interface name>

DESCRIPTION
airtun-ng creates a virtual tunnel interface (atX) for sending arbitrary IP packets by using raw ieee802.11 packet injection.

OPTIONS

-H, --help
    Shows the help screen.

-x <pps>
    Sets maximum number of packets per second.

-a <BSSID>
    Specifies the BSSID for the iee802.11 header.

-h <SMAC>
    Specifies the source MAC for the iee802.11 header.

-i <iface>
    Sets the capture interface.

-r <file>
    Specifies a file to read 802.11 frames.

-y <PRGA-file>
    Is the name of the file, which provides the keystream for WEP encoding. (No receiving, just transmitting of IP packets.)

-w <WEP-key>
    This is the WEP key to en-/decrypt all traffic going through the tunnel.

-t <tods>
    Defines the ToDS and FromDS bit in the ieee802.11 header. For tods=1, the ToDS bit is set to 1 and FromDS to 0, while tods=0 sets them the other way around.

-m <netmask>, --netmask <netmask>
    Filters networks based on bssid ^ netmask combination. Needs -d, used in replay mode.

-d <BSSID>, --bssid <BSSID>
    Filters networks based on the <BSSID>. Used in replay mode.

-f, --repeat
    Enables replay mode. All read frames, filtered by bssid and netmask (if specified), will be replayed.

EXAMPLES
airtun-ng -a 00:14:22:56:F3:4E -t 0 -y keystream.xor wlan0

SEE ALSO
aircrack-ng(1)
airdecap-ng(1)
airdriver-ng(1)
aireplay-ng(1)
airmon-ng(1)
airodump-ng(1)
airolib-ng(1)
airsev-ng(1)
buddy-ng(1)
easside-ng(1)
ivstools(1)
kstats(1)
makeivs-ng(1)
packetforge-ng(1)
wesside-ng(1)