; DAYTEK.INF
;
; This is a Setup information file for DAYTEK monitors.
;
;                                           Version 1.0
;                                           Revision 3.0
;                                           1997. 12.16.

[version]
LayoutFile=layout.inf
signature="$CHICAGO$"
Class=Monitor
Provider=%MS%

;-------------------------------------------------
; Manufacturers

[Manufacturer]
%DAYTEK%=DAYTEK

;-------------------------------------------------
; Driver sections

[DAYTEK]
%DT-1436%=DT-1436, Monitor
%DT-1436A%=DT-1436A, Monitor
%DT-1436AM4%=DT-1436AM4, Monitor
%DT-1436D%=DT-1436D, Monitor
%DT-1436DM2%=DT-1436DM2, Monitor
%DT-1436M2%=DT-1436M2, Monitor
%DT-14SN%=DT-14SN, Monitor
%DT-14SNI%=DT-14SNI, Monitor
%DT-14SNIE%=DT-14SNIE, Monitor
%DT-14ST39%=DT-14ST39, Monitor
%DT-14SV2%=DT-14SV2, Monitor
%DT-14SV3%=DT-14SV3, Monitor
%DT-14VN%=DT-14VN, Monitor
%DT-14WN4%=DT-14WN4, Monitor
%DT-14XV MPR-II%=DT-14XV MPR-II, Monitor
%DT-14XV%=DT-14XV, Monitor
%DT-14XVB%=DT-14XVB, Monitor
%DT-1530%=DT-1530, Monitor
%DT-1531%=DT-1531, Monitor
%DT-1531D%=DT-1531D, Monitor
%DT-1531DB%=DT-1531DB, Monitor
%DT-1536%=DT-1536, Monitor
%DT-1536A%=DT-1536A, Monitor
%DT-1536D%=DT-1536D, Monitor
%DT-1726D%=DT-1726D, Monitor
%DT-1730%=DT-1730, Monitor
%DT-1731%=DT-1731, Monitor
%DT-1731D%=DT-1731D, Monitor
%DT-1731DB%=DT-1731DB, Monitor
;-------------------------------------------------
; Install sections

;--------------- DAYTEK
[DT-1436]
DelReg=Del_Current_REG
AddReg=Res_48K.AddReg, 1024, DPMS
[DT-1436A]
DelReg=Del_Current_REG
AddReg=Res_48K.AddReg, 1024, DPMS
[DT-1436AM4]
DelReg=Del_Current_REG
AddReg=Res_48K.AddReg, 1024, DPMS
[DT-1436D]
DelReg=Del_Current_REG
AddReg=Res_48K.AddReg, 1024, DPMS
[DT-1436DM2]
DelReg=Del_Current_REG
AddReg=Res_54K.AddReg, 1024, DPMS
[DT-1436M2]
DelReg=Del_Current_REG
AddReg=Res_48K.AddReg, 1024, DPMS
[DT-14SN]
DelReg=Del_Current_REG
AddReg=Res_38K.AddReg, 1024
[DT-14SNI]
DelReg=Del_Current_REG
AddReg=Res_48K.AddReg, 1024
[DT-14SNIE]
DelReg=Del_Current_REG
AddReg=Res_48K.AddReg, 1024, DPMS
[DT-14ST39]
DelReg=Del_Current_REG
AddReg=Res_38K.AddReg, 1024
[DT-14SV2]
DelReg=Del_Current_REG
AddReg=Res_SVGA.AddReg, 1024
[DT-14SV3]
DelReg=Del_Current_REG
AddReg=Res_SVGA.AddReg, 1024
[DT-14VN]
DelReg=Del_Current_REG
AddReg=Res_VGA.AddReg, 640
[DT-14WN4]
DelReg=Del_Current_REG
AddReg=Res_VGA.AddReg, 640
[DT-14XV MPR-II]
DelReg=Del_Current_REG
AddReg=Res_56K.AddReg, 1024, DPMS
[DT-14XV]
DelReg=Del_Current_REG
AddReg=Res_56K.AddReg, 1024, DPMS
[DT-14XVB]
DelReg=Del_Current_REG
AddReg=Res_56K.AddReg, 1024, DPMS
[DT-1530]
DelReg=Del_Current_REG
AddReg=Res_64K.AddReg, 1280, DPMS
[DT-1531]
DelReg=Del_Current_REG
AddReg=Res_69K.AddReg, 1280, DPMS
[DT-1531D]
DelReg=Del_Current_REG
AddReg=Res_69K.AddReg, 1280, DPMS
[DT-1531DB]
DelReg=Del_Current_REG
AddReg=Res_69K.AddReg, 1280, DPMS
[DT-1536]
DelReg=Del_Current_REG
AddReg=Res_48K.AddReg, 1024, DPMS
[DT-1536A]
DelReg=Del_Current_REG
AddReg=Res_48K.AddReg, 1024, DPMS
[DT-1536D]
DelReg=Del_Current_REG
AddReg=Res_54K.AddReg, 1024, DPMS
[DT-1726D]
DelReg=Del_Current_REG
AddReg=Res_69K.AddReg, 1280, DPMS
[DT-1730]
DelReg=Del_Current_REG
AddReg=Res_64K.AddReg, 1280, DPMS
[DT-1731]
DelReg=Del_Current_REG
AddReg=Res_64K.AddReg, 1280, DPMS
[DT-1731D]
DelReg=Del_Current_REG
AddReg=Res_69K.AddReg, 1280, DPMS
[DT-1731DB]
DelReg=Del_Current_REG
AddReg=Res_69K.AddReg, 1280, DPMS

; Common AddReg sections

[Del_Current_REG]
HKR,MODES
HKR,,MaxResolution

[640]
HKR,,MaxResolution,,"640,480"
[800]
HKR,,MaxResolution,,"800,600"
[1024]
HKR,,MaxResolution,,"1024,768"
[1152]
HKR,,MaxResolution,,"1152,870"
[1280]
HKR,,MaxResolution,,"1280,1024"
[1600]
HKR,,MaxResolution,,"1600,1200"

[DPMS]
HKR,,DPMS,,1

;-------------------------------------------------
; Model AddReg sections

; -------------- DAYTEK
[Res_VGA.AddReg]
HKR,"MODES\640,350",Mode1,,"31.5,70.1,+,-"
HKR,"MODES\640,400",Mode2,,"31.5,70.1,-,+"
HKR,"MODES\640,480",Mode3,,"31.5,60.0,-,-"
HKR,,ICMProfile,1,9

[Res_SVGA.AddReg]
HKR,"MODES\640,350",Mode1,,"31.5,70.1,+,-"
HKR,"MODES\640,400",Mode2,,"31.5,70.1,-,+"
HKR,"MODES\640,480",Mode3,,"31.5,60.0,-,-"
HKR,"MODES\640,480",Mode4,,"35.0,66.7,+,-"
HKR,"MODES\800,600",Mode5,,"35.2,56.3,+,+"
HKR,"MODES\1024,768",Mode6,,"35.5,87.0,+,+"
HKR,,ICMProfile,1,9
[Res_38K.AddReg]
HKR,"MODES\800,600",Mode1,,"30-39,50-90,+,+"
HKR,,ICMProfile,1,8
[Res_48K.AddReg]
HKR,"MODES\1024,768",Mode1,,"30-49,50-100,+,+"
HKR,,ICMProfile,1,8
[Res_54K.AddReg]
HKR,"MODES\1024,768",Mode1,,"30-55,50-110,+,+"
HKR,,ICMProfile,1,8
[Res_56K.AddReg]
HKR,"MODES\1024,768",Mode1,,"30-57,50-90,+,+"
HKR,,ICMProfile,1,8
[Res_64K.AddReg]
HKR,"MODES\1280,1024",Mode1,,"30-65,50-90,+,+"
HKR,,ICMProfile,1,8
[Res_69K.AddReg]
HKR,"MODES\1280,1024",Mode1,,"30-70,50-120,+,+"
HKR,,ICMProfile,1,8

;-------------------------------------------------
; User visible strings

[Strings]
MS="Microsoft"

;----------------- DAYTEK
DAYTEK="DAYTEK"

DT-1436="DAYTEK DT-1436"
DT-1436A="DAYTEK DT-1436A"
DT-1436AM4="DAYTEK DT-1436AM4"
DT-1436D="DAYTEK DT-1436D"
DT-1436DM2="DAYTEK DT-1436DM2"
DT-1436M2="DAYTEK DT-1436M2"
DT-14SN="DAYTEK DT-14SN"
DT-14SNI="DAYTEK DT-14SNI"
DT-14SNIE="DAYTEK DT-14SNIE"
DT-14ST39="DAYTEK DT-14ST39"
DT-14SV2="DAYTEK DT-14SV2"
DT-14SV3="DAYTEK DT-14SV3"
DT-14VN="DAYTEK DT-14VN"
DT-14WN4="DAYTEK DT-14WN4"
DT-14XV MPR-II="DAYTEK DT-14XV MPR-II"
DT-14XV="DAYTEK DT-14XV"
DT-14XVB="DAYTEK DT-14XVB"
DT-1530="DAYTEK DT-1530"
DT-1531="DAYTEK DT-1531"
DT-1531D="DAYTEK DT-1531D"
DT-1531DB="DAYTEK DT-1531DB"
DT-1536="DAYTEK DT-1536"
DT-1536A="DAYTEK DT-1536A"
DT-1536D="DAYTEK DT-1536D"
DT-1726D="DAYTEK DT-1726D"
DT-1730="DAYTEK DT-1730"
DT-1731="DAYTEK DT-1731"
DT-1731D="DAYTEK DT-1731D"
DT-1731DB="DAYTEK DT-1731DB"