;//////////////////////////////////////////////////
;VP5083 dirver-------------video inf
///////////////////////////////////////////////////

[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="Twinhan"
DriverVer=07/25/2005,0.0.1.1
[Manufacturer]
"Twinhan"=Twinhan

[SourceDisksNames]
1="Twinhan VP5083 Drivers",,,""

[SourceDisksFiles]
TV5083vid.sys=1

[Twinhan]
; motorola(mc801) tuner & tda9887(all standard)
%CX23880.videoMoto%=CX23880.Motorola,PCI\VEN_14F1&DEV_8800&SUBSYS_00201822


[DestinationDirs]
CX23880.CopyDrivers=10,system32\drivers
CX23880.CopyFilters=11

[CX23880.CopyDrivers]
TV5083vid.sys

[CX23880.CopyFilters]
; none for now


[CX23880.Motorola]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Motorola.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters

[CX23880.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,cx88vid.sys
HKR,,OkToHibernate,3,01
HKR,,PageOutWhenUnopened,3,00
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKR,"DriverData","XBarInPin0",0x00010001, 0x03,0x00,0x00,0x00
HKR,"DriverData","XBarInPin1",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","XBarInPin2",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData","XBarInPin3",0x00010001, 0x00,0x10,0x00,0x00
HKR,"DriverData","XTal0",0x00010001, 0x1c, 0x00, 0x00, 0x00
HKR,"DriverData","XTal1",0x00010001, 0x23, 0x00, 0x00, 0x00
HKR,"DriverData","BobMode",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","VolumeLevelNegdB",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","UseExternalVPRES",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","UseI2SAsClock",0x00010001, 0x00, 0x00, 0x00, 0x00


[Motorola.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"ENUM\Device1",pnpid,,"cxtune.VEN_14F1.Motorola"
HKR,"ENUM\Device2",pnpid,,"cx88xbar.VEN_14F1.Motorola"

[VideoCapture]
AddReg=VideoCapture.AddReg

[VideoTvAudio]
AddReg=VideoTvAudio.AddReg

[VideoCapture.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%CX23880.friendly%

[VideoTvAudio.AddReg]
HKR,,CLSID,,{71F96462-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%CX23880.friendly2%

[CX23880.Motorola.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.Motorola.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.ServiceInstall]
DisplayName   = %CX23880.video%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_AUTO_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\system32\drivers\TV5083vid.sys

[Strings]
CX23880.video               = "VP5083 Video Capture"
CX23880.friendly            = "VP5083 Video Capture"
CX23880.friendly2           = "VP5083 TvAudio"
CX23880.videoMoto	    = "VP5083 Video"
;RunOnce                    = "SOFTWARE\Microsoft\Windows\CurrentVersion\RunOnce"
SERVICE_KERNEL_DRIVER       = 1
SERVICE_AUTO_START          = 2
SERVICE_ERROR_NORMAL        = 1


